**Industrial Panel code review**

**Tasks**

The panel have three main tasks, one for LVGL(screen), other for sensors, and other for http server.

|  |
| --- |
| **static** **void** **main\_task**(**void** \*arg)  {  vTaskSetApplicationTaskTag( NULL, ( **void** \* ) 1);/\*Task Tag\*/  LWIP\_UNUSED\_ARG(arg);  stack\_init();  http\_server\_socket\_init();  **while**(1)  {  update\_server\_sensors();  vTaskDelay(40);  }  vTaskDelete(NULL);  } |
| **static** **void** **UpdateSensorTask**(**void** \*param)  {  vTaskSetApplicationTaskTag( NULL, ( **void** \* ) 3);/\*Task Tag\*/  **while**(false == g\_gui\_guider\_init);  **for** (;;)  {  update\_values();  motor\_control\_task();  vTaskDelay(40);  }  } |
| **static** **void** **AppTask**(**void** \*param)  {  vTaskSetApplicationTaskTag( NULL, ( **void** \* ) 2);/\*Task Tag\*/  **#if** LV\_USE\_LOG  lv\_log\_register\_print\_cb(print\_cb);  **#endif**  lv\_init();  lv\_port\_disp\_init();  lv\_port\_indev\_init();  s\_lvgl\_initialized = true;  setup\_ui(&guider\_ui);  events\_init(&guider\_ui);  custom\_init(&guider\_ui);  g\_gui\_guider\_init = true;  **for** (;;)  {  lv\_task\_handler();  update\_screen\_values(&guider\_ui);  vTaskDelay(40);  }  } |

**Sensors and dynamic parts**

All of this are in “sensors” source folder, here is two files, header and source.

The data that sensor module manage are CPU performance, touch sensitivity, real time clock (rtc), CPU temperature, board temperature, rpm of motor and counter (control interface). Also allow to check data updates for lvgl and server.

Next one are typedef structs and enumerations

|  |
| --- |
| **typedef** **struct** \_performance\_data\_t  {  uint8\_t server\_task\_int;  uint8\_t lvgl\_task\_int;  uint8\_t other\_task\_int;  uint8\_t idle\_task\_int;  uint8\_t server\_task\_tens;  uint8\_t lvgl\_task\_tens;  uint8\_t other\_task\_tens;  uint8\_t idle\_task\_tens;  } performance\_data\_t; |
| **typedef** **struct** \_touch\_sensitive\_data\_t  {  uint16\_t touch\_sensitive\_data;  uint8\_t touch\_sensitive\_percentaje;  } touch\_sensitive\_data\_t; |
| **typedef** **struct** \_rtc\_data\_t  {  uint8\_t day;  uint8\_t month;  uint16\_t year;  uint8\_t hours;  uint8\_t minutes;  uint8\_t seconds;  } rtc\_data\_t; |
| **typedef** **struct** \_temperature\_data\_t  {  uint8\_t internal\_temperature;  uint8\_t external\_temperature;  } temperature\_data\_t; |
| **typedef** **struct** \_control\_interface\_values\_t  {  uint16\_t rpm;  uint16\_t counter;  } control\_interface\_values\_t; |
| **typedef** **struct** \_sensor\_updates\_t  {  bool update\_ext\_temperature;  bool update\_mcu\_temperature;  bool update\_performance;  bool update\_rtc;  bool update\_touch;  } sensor\_updates\_t; |

Now function prototypes

|  |
| --- |
| /\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*  @brief : This function convert integer to string  @param : value -> Integer value to convert  @param : string -> Buffer pointer to save string number  @param : int\_len -> String length, if is more than number need is filled with '0'  @return: Return sign of number (Not put '-' in string)  \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/  sign\_of\_string\_t **int\_to\_string**(int32\_t value, uint8\_t\* string, uint8\_t int\_len);  // ----------------------------------------------------------------------------------------- |
| /\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*  @brief : This function convert string to integer.  @param : buffer -> String to convert, support negative number "-00050" or "-50" or "50"  @param : size -> Size of string  @return: Integer number  \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/  int32\_t **string\_to\_int**(uint8\_t buffer[], uint8\_t size);  // ------------------------------------------------------------------------------------------ |
| /\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*  @brief : This function is for lvgl, if some value is updated this returns true  @return: True if some value is updated, false if not  \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/  bool **sensor\_updates\_screen**();  // ------------------------------------------------------------------------------------------ |
| /\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*  @brief : This function is for server, if some value is updated this returns true  @return: True if some value is updated, false if not  \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/  bool **sensor\_updates\_server**();  // ------------------------------------------------------------------------------------------ |
| /\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*  @brief : This indicate values that are updated for lvgl (used for performance)  @return: struct with flags that indicate updated values  \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/  sensor\_updates\_t **get\_values\_state\_screen**();  // ------------------------------------------------------------------------------------------ |
| /\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*  @brief : This indicate values that are updated for server (used for performance)  @return: struct with flags that indicate updated values  \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/  sensor\_updates\_t **get\_values\_state\_server**();  // ------------------------------------------------------------------------------------------ |
| /\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*  @brief : Here get values of CPU performance  @return: struct that have all CPU performance data, integer and tens are separated  \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/  performance\_data\_t **get\_performance\_data**();  // ------------------------------------------------------------------------------------------ |
| /\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*  @brief : Here get values of touch sensitive sensor  @return: struct that have touch sensitive data  \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/  touch\_sensitive\_data\_t **get\_touch\_sensitive\_data**();  // ------------------------------------------------------------------------------------------ |
| /\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*  @brief : Here get values of real time clock (RTC)  @return: struct with all RTC values  \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/  rtc\_data\_t **get\_rtc\_data**();  // ------------------------------------------------------------------------------------------ |
| /\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*  @brief : Here get temperature values (board and CPU)  @return: struct with both temperature values  \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/  temperature\_data\_t **get\_temperature\_data**();  // ------------------------------------------------------------------------------------------ |
| /\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*  @brief : Here get values of control interface panel (rpm and counter)  @return: struct with rpm and counter  \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/  control\_interface\_values\_t **get\_control\_interface\_data**();  // ------------------------------------------------------------------------------------------ |
| /\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*  @brief : This function allows to set rpm between (0, 4000), if is less than 500 is set to 0  @param : rpm -> Desired rpm  @return: None  \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/  **void** **set\_rpm**(uint16\_t rpm);  // ------------------------------------------------------------------------------------------ |
| /\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*  @brief : This function allows to get desired rpm  @return: Actual desired rpm  \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/  uint16\_t **get\_rpm**();  // ------------------------------------------------------------------------------------------ |
| /\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*  @brief : Increment control interface counter  @return: None  \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/  **void** **increment\_counter**();  // ------------------------------------------------------------------------------------------ |
| /\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*  @brief : Decrement control interface counter  @return: None  \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/  **void** **decrement\_counter**();  // ------------------------------------------------------------------------------------------ |
| /\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*  @brief : Periodic function used for update all values, called for "other" task in main  @return: None  \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/  **void** **update\_values**();  // ------------------------------------------------------------------------------------------ |

**LVGL (graphics on screen)**

Here use default functions created from gui guider, but we create other that update screen values form sensor values, the function is “update\_screen\_values”.

**Web panel**

Server is managed with request, html make a request and the uC response with data array that is modified by function “update\_server\_sensors”